**TERMS OF REFERENCE**

**for the purchase of water trucks to supply water to drill rigs of the Drill/Blast Department**

|  |  |  |
| --- | --- | --- |
| **Item**  **№** | **List of basic**  **data and requirements** | **Basic data and requirements** |
| 1 | Equipment delivery location | Issyk-Kul Region, Jeti-Oguz District, Kumtor Gold Mine |
| 2 | Client | Kumtor Gold Company CJSC |
| 3 | Purpose | The purpose of this ToR is to purchase 2 units of water trucks to supply water to the Drill/Blast drill rigs in operating conditions of the Kumtor open pits. |
| 4 | Requirements for the vehicle | * Vehicle type: truck with water tank. * Wheel configuration: 6x4 or 6x6, depending on the operating conditions. The 6x6 model is preferred for difficult terrain. * Tank volume: 10-16 cubic metres. * Chassis: the load chassis shall be adapted for the tank installation, considering the load and dimensions. * Overall dimensions: shall not exceed the maximum permissible limits for public roads. * Year of manufacture: 2022-2024. * Quantity - 2 units. * Preferred brands of water truck chassis are KAMAZ, HOWO (Sinotruck), ISUZU, FAW, HYUNDAI, HINO. |
| 5 | Requirements for the tank | * Material: steel with anti-corrosion coating or stainless steel to prevent corrosion. * Insulation: if possible, thermal insulation of the tank to prevent water freezing at low temperatures. * Pumping equipment: availability of a pump to supply pressurized water with the possibility to fill both horizontally and vertically positioned tanks. * Hatches: top and bottom hatches for easy filling and maintenance. * Drain and pressure system: drain system with quick connection for hoses of various diameters. * Heating system: tanks shall be equipped with heating to prevent water freezing in winter (up to -40 oC). |
| 6 | Technical specifications | * Engine: diesel engine with an output of at least 300 hp, complying with environmental safety standards (not lower than Euro-4). * Transmission: manual, with reinforced transmission for off-road use. * Drive: all-wheel drive or rear-wheel drive, depending on the wheel configuration. * Fuel tank: increased capacity for long trips without refueling, at least 300 liters. * Maximum speed: max. 80 km/h. * Ground clearance: high for difficult terrain. |
| 7 | Operating conditions | * Temperature range: -40°C to +27°C. * Road conditions: driving on steep climbs, off-road is possible. |
| 8 | Configuration requirements | * Driver's cab: equipped for comfortable operation, with air conditioning and heater. * Safety system: availability of seat belts, ABS, and stabilization system. * Tools and spare parts: minimum set of tools for maintenance and operation. |
| 9 | Warranty obligations | * Vehicle warranty: at least 2 years or 100,000 kilometers of mileage. * Tank and pumping equipment warranty: at least 2 years. * Maintenance: frequency of maintenance and service in the region of operation. |
| 10 | Requirements for spare parts availability | * Supplier shall ensure stock availability of main spare parts for water trucks during the whole warranty period. * Obligation to supply spare parts at the Client's request within no more than 30 calendar days from the receipt of the purchase order. * Spare parts shall be original or equivalent in quality, with appropriate certificates. * Supplier shall provide a list of spare parts and consumables that may be required for routine maintenance and repairs. |
| 10 | Documentation | * Vehicle passport. * Water truck operation manual. * Certificates of Conformity. |
| 11 | Additional requirements | * Vehicles proposed shall be new, not used, certified, or declared, fully compliant with quality standards, certificate of conformity. * Vehicles shall not be pledged, arrested, shall be free from the rights of third parties. * Adaptation to specific operating conditions and client's requirements shall be possible. * Training materials for water truck operators shall be provided. |
| 12 | Payment and delivery terms | * Payment terms shall be specified in the agreement. * Delivery terms: no more than 45 calendar days from the date of the agreement. |